|  |  |
| --- | --- |
| **2.0 SEAL KIT NS (sm/co)**  **Dust Seal Cap O-Ring** OR 41x1.78 (AS-030/N70)  **Dust Seal** DTW 20-28-5 (SKF)  **Rod Guide O-Ring** OR 39x4.0 (N70)  **Oil Seal** USH or UP 20-28-5 (NOK)  **O-Ring** OR 19.8-2.4 (VITON 75)  **Valve Body O-Ring** OR-7x2.5  **PRO-2.0-SEALKIT-NS** | **2.5 SEAL KIT NS (sm/co/bp)**  **Dust Seal** DTW 22-30-5 (WPI 22-30-4.5/6 nak)  **Dust Cap O-Ring** OR 56.78x1.78 (AS-035/N70)  **Rod Guide O-Ring** OR 53x4.0 (N70)  **Oil Seal** ZBR or USH 22-30-5 (NOK)  **O-Ring** OR 21.8x2.4 (VITON 75)  **Valve Body O-Ring** OR-7x2.5  **PRO-2.5-SEALKIT-NS** |
| **2.5 AIRSHOX & BUMPSTOP SEAL KIT**  **Dust Seal Cap O-Ring** OR 56.78x1.78 (AS-035/N70)  **Dust Seal** DTW 40-48-5-J2G  **Oil Seal** ZBR 40-50-7-E6W or USH-40-50-6  **Rod Guide Ext O-Ring** OR 53x4.0 (N70)  **Rod Guide Int O-Ring** OR 39.7x3.5 (P40/V75)  **Valve Body O-Ring** OR-7x2.5  **PRO-2.5-ASBS-SEALKIT** | **2.0 SEAL KIT OS (sm/co)**  **Dust Seal** WP4-20-32-6/9  **Oil Seal** UP-20-28-5  **Dust Cap O-Ring** OR 42-1.78 / OR 41-1.78  **Rod Guide O-Ring** OR 39-3.5 / OR 39.7-3.5  **Valve Body O-Ring** OR-7x2.5  **PRO-2.0-SEALKIT-OS** |
| **2.5 SEAL KIT OS (sm/co/bp)**  **Dust Seal** W-22-30-26-9/4  **Oil Seal** U-22-32-8  **Dust Cap O-Ring** OR 56.78-1.78  **Rod Guide Ext O-Ring** OR 53-4  **Rod Guide Int O-Ring** OR 21.67-3.5V / OR 21.82-3.53  **Valve Body O-Ring** OR-7x2.5  **PRO-2.5-SEALKIT-OS** | **2.0 BUMP STOP SEAL KIT ALL**  **Dust Seal** 839N-0320 or DTW-32-40-5-J2G  **Oil Seal** 601N-32-42 or ZBR-32-42-803-E6W  **Rod Guide O-Ring** OR 39-4  **Cap O-Ring** OR 40.94-2.62 (AS130)  **Valve Body O-Ring** OR-7x2.5  **PRO-2.0-BSSK-ALL** |
| **2.5 2-WAY CO LOWER ADJUSTER SEAL KIT**  **Ball Bearing** TF-GRB-4  **Spring** CS-4-2.8-0.6-6  **Cam Valve** AJV-13-8-34  **O-Ring** OR-4.5-1.5  **O-Ring** OR-13.5x1.5 (S14/N70)  **Adj. Valve Stop** AVS-8-M16x1.25-14  **Dust Seal** VC-8-12-3  **PRO-2.5-2WAY-LAK** | **2.5 2-WAY CO UPPER VALVE SEAL KIT**  **Adj. Valve** ASV-8-23.3-5.5  **Spring** SPC-0.8-7.1-5.5-11  **O-Ring x 2** OR 5x1.50  **Nut-Adj. Screw** AS-8-M10x1.0-47  **Nut Lock-Adj. Screw** LSRA-13.5-5-M8x1.0  **PRO-2.5-2WAY-UVK** |